{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["基本信息"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"基本信息","index":0,"n_rows":92,"n_cols":6,"rows_kept":92,"cut":false,"hidden":false,"merged":[[51,2,51,3],[62,2,62,3],[60,4,60,5],[61,4,61,5],[62,4,62,5],[60,0,60,1],[60,2,60,3],[61,0,61,1],[62,0,62,1],[61,2,61,3],[35,4,35,5],[36,4,36,5],[37,4,37,5],[38,4,38,5],[39,4,39,5],[59,4,59,5],[54,4,54,5],[80,4,80,5],[39,0,39,1],[35,2,35,3],[36,2,36,3],[37,2,37,3],[38,2,38,3],[39,2,39,3],[66,4,66,5],[67,4,67,5],[65,4,65,5],[59,0,59,1],[56,2,56,3],[57,2,57,3],[58,2,58,3],[59,2,59,3],[79,4,79,5],[90,0,90,1],[90,3,90,5],[91,0,91,1],[91,3,91,5],[12,0,16,0],[14,1,14,2],[14,4,14,5],[15,1,15,2],[15,4,15,5],[49,0,49,1],[87,0,87,1],[87,4,87,5],[88,0,88,1],[89,0,89,1],[84,0,84,1],[84,4,84,5],[85,0,85,1],[85,4,85,5],[86,0,86,1],[86,4,86,5],[78,0,78,1],[78,2,78,3],[78,4,78,5],[81,0,81,1],[81,2,81,3],[81,4,81,5],[79,0,79,1],[80,0,80,1],[79,2,79,3],[80,2,80,3],[73,4,73,5],[76,0,76,5],[77,0,77,1],[77,2,77,3],[77,4,77,5],[68,4,68,5],[69,4,69,5],[70,4,70,5],[71,4,71,5],[72,4,72,5],[55,0,55,1],[55,2,55,3],[55,4,55,5],[56,4,56,5],[57,4,57,5],[58,4,58,5],[56,0,56,1],[57,0,57,1],[58,0,58,1],[48,0,48,1],[48,2,48,3],[52,0,52,1],[52,2,52,3],[54,0,54,1],[54,2,54,3],[50,0,50,1],[49,2,49,3],[50,2,50,3],[51,0,51,1],[34,0,34,1],[34,2,34,3],[34,4,34,5],[40,0,40,1],[40,2,40,3],[40,4,40,5],[35,0,35,1],[36,0,36,1],[37,0,37,1],[38,0,38,1],[32,0,32,1],[32,2,32,3],[32,4,32,5],[33,0,33,1],[33,2,33,3],[33,4,33,5],[30,0,30,1],[30,2,30,3],[30,4,30,5],[31,0,31,1],[31,2,31,3],[31,4,31,5],[28,0,28,1],[28,2,28,3],[28,4,28,5],[29,0,29,1],[29,2,29,3],[29,4,29,5],[26,0,26,1],[26,2,26,3],[23,0,23,1],[23,2,23,3],[24,0,24,1],[24,2,24,3],[25,0,25,1],[25,2,25,3],[13,1,13,2],[13,4,13,5],[16,1,16,2],[16,4,16,5],[22,0,22,1],[22,2,22,3],[7,1,7,2],[7,4,7,5],[8,1,8,2],[8,4,8,5],[10,1,10,5],[12,1,12,2],[12,4,12,5],[0,0,0,5],[3,1,3,2],[3,4,3,5],[4,1,4,2],[4,4,4,5],[6,1,6,2],[6,4,6,5]],"flags":["formulas_cached_only"]}
["\n广东科士达工业科技有限公司信息公示"]
[]
["基本信息"]
["单位名称：","广东科士达工业科技有限公司",null,"生产地址：","惠州市仲恺高新技术产业开发区35号小区"]
["法定代表人：","刘程宇",null,"组织机构代码：","91441300796251955W"]
[]
["区号：","0752",null,"联系电话：",5751688]
["联系人：","张琳",null,"传真号码：",5751688]
["邮政编码：",516000,null,"企业类型：","有限责任公司（台港澳与境内合资）"]
[]
["生产经营和管理服务的主要内容（经营范围）","生产销售计算机网络和外围设备，UPS和逆变电源产品，动力配电设备、制冷空调设备、金属制品（不含电镀）、防雷产品、太阳能电池和控制器产品、蓄电池产品及相关材料、软件开发及相关技术服务。产品20%外销，80%内销。从事铅酸蓄电池产品的生产设备及有关检测设备的批发零售及进出口业务（不设店铺、不涉及国营贸易管理商品，涉及配额、许可证管理及其他专项规定管理的商品，按国家有关规定办理申请）。（依法须经批准的项目，经相关部门批准后方可开展经营活动。）="]
[]
["主要产品：","产品名称",null,"计量单位","实际年产量"]
[null,"铅酸蓄电池",null,"千伏安时",269000]
[null,"UPS",null,"万台",120]
[null,"整体机房成套设备",null,"套",100000]
[null,"光伏逆变器",null,"台",4284]
[]
["废水污染信息"]
["排放口编号","执行标准","允许排放的总量","分布位置","排放污染物种类","排放去向类型"]
["DW002","电池工业污染物排放标准GB 30484-2013,水污染物排放限值DB44/26-2001","-","厂内污水站","化学需氧量、总铅、氨氮","惠州市第七污水厂"]
[]
["污染物名称",null,"排放标准",null,"排放浓度","排放总量"]
["化学需氧量",null,"90mg/L",null,"53.52406mg/L","0.132365t/年"]
["总铅",null,"0.5mg/L",null,"0.30841mg/L","0.000264t/年"]
["氨氮",null,"10mg/L",null,"2.84998mg/L","0.007048t/年"]
[]
[]
["监测时间",null,"监测报告编号",null,"超标情况"]
["2021.01.25",null,"BHJS2021-0365",null,"达标"]
["2021.02.22",null,"BHJS2021-0627",null,"达标"]
["2021.03.26",null,"BHJS2021-1074",null,"达标"]
["2022.04.23",null,"BHJS2021-1392",null,"达标"]
["2021.05.25",null,"BHJS2021-1830",null,"达标"]
["2021.06.28",null,"BHJS2021-2335",null,"达标"]
["2021.07.19",null,"BHJS2021-2759",null,"达标"]
["2021.08.31",null,"BHJS2021-3418",null,"达标"]
["2021.09.23",null,"BHJS2021-3701",null,"达标"]
["2021.10.30",null,"BHJS2021-4222",null,"达标"]
["2021.11.29",null,"BHJS2021-4504",null,"达标"]
["2021.12.31",null,"BHJS2022-0050",null,"达标"]
[]
["废气污染信息"]
["排放口编号","执行标准","允许排放的总量","分布位置","排放污染物种类","排放去向类型"]
["DA003、DA004、DA006A、DA007、DA008、DA009","《电池工业污染物GB》（30484-2013）表5排放限值","0.03228吨/年","厂内","铅及其化合物","达标排放"]
["DA006B","印刷行业挥发性有机化合物排放标准(DB44/815-2010)丝网印刷标准","-","厂内","总挥发性有机物","达标排放"]
["DA001、DA002、DA010","《电池工业污染物GB》（30484-2013）表5排放限值","-","厂内","硫酸雾","达标排放"]
[]
["污染物名称",null,"排放标准",null,"排放浓度","排放总量"]
["硫酸雾",null,"5mg/Nm³",null,"达标","/"]
["总挥发性有机物",null,"120mg/Nm³",null,"达标","/"]
["铅及其化合物",null,"0.5mg/Nm³",null,"0.04mg/m3","0.686986KG/年"]
[]
[]
["监测时间",null,"监测报告编号",null,"超标情况"]
["2021.01.25-26",null,"BHJQ2021-0137",null,"达标"]
["2021.02.22-23",null,"BHJQ2021-0207",null,"达标"]
["2021.03.26-27",null,"BHJQ2021-0371",null,"达标"]
["2021.04.23、25",null,"BHJQ2021-0506",null,"达标"]
["2021.05.25",null,"BHJQ2021-0657",null,"达标"]
["2021.06.16",null,"BHJQ2021-0801",null,"达标"]
["2021.10.25",null,"BHJQ2021-1456",null,"达标"]
["2021.12.24",null,"BHJQ2021-1868",null,"达标"]
[]
["危险废物信息"]
["废物名称","产生量（单位：吨）","贮存量","规范转移量","倾倒丢弃量"]
["废灯管",0.1,0,0.1,0]
["废活性炭",0.6,0,0.6,0]
["含铅污泥",25.984,0,25.984,0]
["废铅酸蓄电池",411.387,0,411.387,0]
["废矿物油",0.15,0.5,0.1,0]
["废办公用品",0.059,0,0.059,0]
["废空桶",0.07,0,0.07,0]
["废液",0.06,0,0.06,0]
[]
["噪声污染物信息"]
["噪声执行标准：《工业企业厂界噪声标准》（GB12348-2008）3类标准"]
["监测时间",null,"监测报告编号",null,"超标情况"]
["2021.01.26",null,"BHJZ2021-0057",null,"达标"]
["2021.04.25",null,"BHJZ2021-0395",null,"达标"]
["2021.07.19",null,"BHJZ2021-0712",null,"达标"]
["2021.10.25",null,"BHJQ2021-1018",null,"达标"]
[]
["建设项目环境影响评价及其他环境保护行政许可情况"]
["许可文件",null,"批复单位","批复日期","批复编号"]
["关于广东科士达工业科技有限公司环境影响报告书的批复",null,"惠州市环境保护局","2008.04.16","惠市环建〔2008〕J063号"]
["关于广东科士达工业科技有限公司扩建项目环境影响报告书的批复",null,"惠州市环境保护局","2018.05.15","惠市环(仲恺）建〔2018〕37号"]
["国家排污许可证",null,"惠州市生态环境局","2019.09.26","91441300796251955W001Q"]
[]
["突发环境事件应急预案"]
["预案编制情况",null,"备案编号","编制文本"]
["已编制",null,"441325-2021-216-L","KSD-预案-2021见附件"]